A 16 bit

ADD

MUX

17-bit result bus 1st 16 bit

16 bit output

B 16 bit

0

overFlow

1

Result[16]